Radiusd –X output:

rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=124, length=127
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	EAP-Message = 0x0200000b0177617373696d
	Message-Authenticator = 0xe3989752d3fcb1b5b1d08100b3d9be1a
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 0 length 11
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
[files] users: Matched entry wassim at line 1
++[files] returns ok
[ldap] performing user authorization for wassim
[ldap] 	expand: %{Stripped-User-Name} -> 
[ldap] 	... expanding second conditional
[ldap] 	expand: %{User-Name} -> wassim
[ldap] 	expand: (uid=%{%{Stripped-User-Name}:-%{User-Name}}) -> (uid=wassim)
[ldap] 	expand: o=navbey.com, dc=navbey,dc=com -> o=navbey.com, dc=navbey,dc=com
  [ldap] ldap_get_conn: Checking Id: 0
  [ldap] ldap_get_conn: Got Id: 0
  [ldap] performing search in o=navbey.com, dc=navbey,dc=com, with filter (uid=wassim)
  [ldap] object not found
[ldap] search failed
  [ldap] ldap_release_conn: Release Id: 0
++[ldap] returns notfound
++[expiration] returns noop
++[logintime] returns noop
[pap] WARNING: Auth-Type already set.  Not setting to PAP
++[pap] returns noop
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] EAP Identity
[eap] processing type md5
rlm_eap_md5: Issuing Challenge
++[eap] returns handled
Sending Access-Challenge of id 124 to 192.168.1.8 port 1645
	Tunnel-Medium-Type:1 = IEEE-802
	Tunnel-Type:1 = VLAN
	Tunnel-Private-Group-Id:1 = "100"
	EAP-Message = 0x010100160410cdfc8807eda33dfb22ecb9707959c501
	Message-Authenticator = 0x00000000000000000000000000000000
	State = 0x11f1e0c911f0e43d9fb503cbe961a6a6
Finished request 9.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=125, length=140
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	State = 0x11f1e0c911f0e43d9fb503cbe961a6a6
	EAP-Message = 0x020100060315
	Message-Authenticator = 0xb7f9f108a96d5cac942c3380dee724d0
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 1 length 6
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
[files] users: Matched entry wassim at line 1
++[files] returns ok
[ldap] performing user authorization for wassim
[ldap] 	expand: %{Stripped-User-Name} -> 
[ldap] 	... expanding second conditional
[ldap] 	expand: %{User-Name} -> wassim
[ldap] 	expand: (uid=%{%{Stripped-User-Name}:-%{User-Name}}) -> (uid=wassim)
[ldap] 	expand: o=navbey.com, dc=navbey,dc=com -> o=navbey.com, dc=navbey,dc=com
  [ldap] ldap_get_conn: Checking Id: 0
  [ldap] ldap_get_conn: Got Id: 0
  [ldap] performing search in o=navbey.com, dc=navbey,dc=com, with filter (uid=wassim)
  [ldap] object not found
[ldap] search failed
  [ldap] ldap_release_conn: Release Id: 0
++[ldap] returns notfound
++[expiration] returns noop
++[logintime] returns noop
[pap] WARNING: Auth-Type already set.  Not setting to PAP
++[pap] returns noop
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP NAK
[eap] EAP-NAK asked for EAP-Type/ttls
[eap] processing type tls
[tls] Initiate
[tls] Start returned 1
++[eap] returns handled
Sending Access-Challenge of id 125 to 192.168.1.8 port 1645
	Tunnel-Medium-Type:1 = IEEE-802
	Tunnel-Type:1 = VLAN
	Tunnel-Private-Group-Id:1 = "100"
	EAP-Message = 0x010200061520
	Message-Authenticator = 0x00000000000000000000000000000000
	State = 0x11f1e0c910f3f53d9fb503cbe961a6a6
Finished request 10.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=126, length=190
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	State = 0x11f1e0c910f3f53d9fb503cbe961a6a6
	EAP-Message = 0x020200381500160301002d01000029030105383b34d8bec8c2148706793b9a6b60009790aee2f7642620e3efbbeb301cbf000002000a0100
	Message-Authenticator = 0xf2e8b4ef2356e3e96359a1161c24617f
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 2 length 56
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/ttls
[eap] processing type ttls
[ttls] Authenticate
[ttls] processing EAP-TLS
[ttls] eaptls_verify returned 7 
[ttls] Done initial handshake
[ttls]     (other): before/accept initialization
[ttls]     TLS_accept: before/accept initialization
[ttls] <<< TLS 1.0 Handshake [length 002d], ClientHello  
[ttls]     TLS_accept: SSLv3 read client hello A
[ttls] >>> TLS 1.0 Handshake [length 002a], ServerHello  
[ttls]     TLS_accept: SSLv3 write server hello A
[ttls] >>> TLS 1.0 Handshake [length 085e], Certificate  
[ttls]     TLS_accept: SSLv3 write certificate A
[ttls] >>> TLS 1.0 Handshake [length 0004], ServerHelloDone  
[ttls]     TLS_accept: SSLv3 write server done A
[ttls]     TLS_accept: SSLv3 flush data
[ttls]     TLS_accept: Need to read more data: SSLv3 read client certificate A
In SSL Handshake Phase 
In SSL Accept mode  
[ttls] eaptls_process returned 13 
++[eap] returns handled
Sending Access-Challenge of id 126 to 192.168.1.8 port 1645
	EAP-Message = 0x0103040015c00000089b160301002a0200002603014f978dcc5e2751233c20ff09b81a3be08c5344bf5278b073e921ed43d21130c900000a00160301085e0b00085a0008570003a6308203a23082028aa003020102020101300d06092a864886f70d0101050500308193310b3009060355040613024652310f300d060355040813065261646975733112301006035504071309536f6d65776865726531153013060355040a130c4578616d706c6520496e632e3120301e06092a864886f70d010901161161646d696e406578616d706c652e636f6d312630240603550403131d4578616d706c6520436572746966696361746520417574686f72697479
	EAP-Message = 0x301e170d3132303431393035323632305a170d3132303631383035323632305a307c310b3009060355040613024652310f300d0603550408130652616469757331153013060355040a130c4578616d706c6520496e632e312330210603550403131a4578616d706c65205365727665722043657274696669636174653120301e06092a864886f70d010901161161646d696e406578616d706c652e636f6d30820122300d06092a864886f70d01010105000382010f003082010a0282010100d8e5bb5cefd0db1624fbbcbba0a02f4d2b23a12f9f0ea9d1f96dc0ef3a08536f4096b8cb434aac77b625bb7610ea5eafdcba502cc3c094f74c16743d6ec1
	EAP-Message = 0x6f4a8104cc5b98ea30fb86287bf0906ed458604e63412a6339c8bf25fd7f627131a6219db5e5d5f56460df027982eb5b1ca3b59a2fd27666fb7016df166162fe720c659f959cb04266ced87b083b6641a431d002b996fdb4c342b0205c9d2d70878caebee08fc19402b6867af343fe3a43a740bc44c66fcf993bc6c9812377983bcee8f5562d0974abc6142d95c3d582403fcf5dd9d5403fca88bb28eaec1cddafe9d23d1d17e804eb15da303e169756418be76cb204ce0c8bcbe428ceb75995cd2b0203010001a317301530130603551d25040c300a06082b06010505070301300d06092a864886f70d010105050003820101009e6cc83de144237e09
	EAP-Message = 0xce61668125af89da7f9d0dc727464fb50a1a8519ba3eed74c9553738541642751ece1617a2f1f567741ce6ce7e2bec8a2dd7871058ec5c440fc9342fa040dff416cddda61f48137d54fcf6725f487093947b9a02697e2ebf41962618b94e2a4453a1b43f1eacd51657b5407400d2404423f719e9b3779d6936d3b739599586f4ee8138bfac0cce760d17db9072576cea1ae391b95968c7ac2563f4f578a0dbee4750ef50e137a2e998ee6d9e7ea5050688e73a971905e1d468a04f8229c7fc1736cf8ee216f942a6a08790e49070f85fad784a5220f2ef9c99b0bd281d6486d5e8f699c843af9d57a10bc1a4a3d57bc470785d8736c7860004ab308204
	EAP-Message = 0xa73082038fa0030201020209
	Message-Authenticator = 0x00000000000000000000000000000000
	State = 0x11f1e0c913f2f53d9fb503cbe961a6a6
Finished request 11.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=127, length=140
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	State = 0x11f1e0c913f2f53d9fb503cbe961a6a6
	EAP-Message = 0x020300061500
	Message-Authenticator = 0xc7bf1c8e01d83731b9b3b2ab5a0787b6
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 3 length 6
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/ttls
[eap] processing type ttls
[ttls] Authenticate
[ttls] processing EAP-TLS
[ttls] Received TLS ACK
[ttls] ACK handshake fragment handler
[ttls] eaptls_verify returned 1 
[ttls] eaptls_process returned 13 
++[eap] returns handled
Sending Access-Challenge of id 127 to 192.168.1.8 port 1645
	EAP-Message = 0x0104040015c00000089b00bcccc1285b561d81300d06092a864886f70d0101050500308193310b3009060355040613024652310f300d060355040813065261646975733112301006035504071309536f6d65776865726531153013060355040a130c4578616d706c6520496e632e3120301e06092a864886f70d010901161161646d696e406578616d706c652e636f6d312630240603550403131d4578616d706c6520436572746966696361746520417574686f72697479301e170d3132303431393035323632305a170d3132303631383035323632305a308193310b3009060355040613024652310f300d0603550408130652616469757331123010
	EAP-Message = 0x06035504071309536f6d65776865726531153013060355040a130c4578616d706c6520496e632e3120301e06092a864886f70d010901161161646d696e406578616d706c652e636f6d312630240603550403131d4578616d706c6520436572746966696361746520417574686f7269747930820122300d06092a864886f70d01010105000382010f003082010a0282010100c2000de5769708aa73a3affa3ae2581583c4882e26f16a18d443e29db8316192c28b219cbb097059526763db5440029da5f07038fb6a904f36e3a41dc25ee2d693730072613aaff090fd98e30623969bc0d43527de8a6e60ecbcfa6672df1f278419f652471cc787c882a1
	EAP-Message = 0x34970210e501a5f008bce3abbcd4de1b5c5da2287cf6af098930a2a46f6c4c68f2db00dc8b8289dfb961b00fb1b8cec26b996c69e2f2a4207cf29afc6e1e7a95599782388b5a5b5a10f961d816e101fdf26cf6062274aef2b443a5c60787edcd755a986de269abf78fde55eae7f450bca4434e6495b264e6db1bce418c8a417739b3bd52739f9ac134c2c9ed6b7bbf4ed479cb33690203010001a381fb3081f8301d0603551d0e0416041410d684dcfea11dfdc1bb500b759373530aa6d64b3081c80603551d230481c03081bd801410d684dcfea11dfdc1bb500b759373530aa6d64ba18199a48196308193310b3009060355040613024652310f300d
	EAP-Message = 0x060355040813065261646975733112301006035504071309536f6d65776865726531153013060355040a130c4578616d706c6520496e632e3120301e06092a864886f70d010901161161646d696e406578616d706c652e636f6d312630240603550403131d4578616d706c6520436572746966696361746520417574686f72697479820900bcccc1285b561d81300c0603551d13040530030101ff300d06092a864886f70d010105050003820101002d0d028da27788c0e5d3623cdb4cf11f09216955fe7493bfa233ec62bb45d3cb9dd71d61a95ca6e1ddb8aa2f8b80fbfcea5b8b35776bc61c9acab1408bc31daf3cf0f27d531819b600d3ca7a7c33
	EAP-Message = 0xf4b1017102971b6ff4eedeea
	Message-Authenticator = 0x00000000000000000000000000000000
	State = 0x11f1e0c912f5f53d9fb503cbe961a6a6
Finished request 12.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=128, length=140
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	State = 0x11f1e0c912f5f53d9fb503cbe961a6a6
	EAP-Message = 0x020400061500
	Message-Authenticator = 0xd0b97ba2bc1d3779f002fc2f1f737d62
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 4 length 6
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/ttls
[eap] processing type ttls
[ttls] Authenticate
[ttls] processing EAP-TLS
[ttls] Received TLS ACK
[ttls] ACK handshake fragment handler
[ttls] eaptls_verify returned 1 
[ttls] eaptls_process returned 13 
++[eap] returns handled
Sending Access-Challenge of id 128 to 192.168.1.8 port 1645
	EAP-Message = 0x010500b915800000089b77cbd7b846662c36009c223bb1dab20d1956c65d6dfdd68e272a551fae0e5b9066339a0f279041f434256e4aa905eb8dbabc508c2a0771d29cb0810ff8a278d32154413350d24a65e9c3cfb9e15e9057d0dce5f2cbd3d523586b6b7f60bf3a6d92c8772b862711d539a2412abe6a6c4f79816985453331bc5f8661a99c795b6d6a92fd75d73273373be417324e2b8696ff3d6cb180e1619343b8bf9d39a193cf49a3f008a74e16030100040e000000
	Message-Authenticator = 0x00000000000000000000000000000000
	State = 0x11f1e0c915f4f53d9fb503cbe961a6a6
Finished request 13.
Going to the next request
Waking up in 4.8 seconds.
rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=129, length=460
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	State = 0x11f1e0c915f4f53d9fb503cbe961a6a6
	EAP-Message = 0x020501441500160301010610000102010073194ca5b531f00b256dce081db91a56312bac8fd142095b2dc51a4c241c135ad86cad0fdbc4d894c26eaf1d30e74cf1f486cc468ee4e06a5c3decee1d71c2c199aef9af6e7ab9588956782adc416c01642324fc70e1b8f717c8f15cb94b96fe5bd46e74fbbd6bf177a9516ffddab869c30a603c80ecb6cfb3f22e767f1207300ecf9485a4f1ca2622d8243a4b374445013c636f86c0b9df7cda38d8bbc72e8272b2735283911709f835a9a9e71cf9ef8d570710882dd7cca1ebc798463bd9915892827b6382d667fdcb8dc87850d62fde397fc8a886a654203c5bd4c1ba3bb3698880b515f23525ca510fd9
	EAP-Message = 0x810d4102d523d13400a57aebb2e280dfdd69337b14030100010116030100289960bba0a0462d1c4fb44f79e13752a8a00a271724a12d4f9a2ec40ea15fcc3968daf29b7317c924
	Message-Authenticator = 0x1ede700171c85bcdd9e593db550969d6
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 5 length 253
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/ttls
[eap] processing type ttls
[ttls] Authenticate
[ttls] processing EAP-TLS
[ttls] eaptls_verify returned 7 
[ttls] Done initial handshake
[ttls] <<< TLS 1.0 Handshake [length 0106], ClientKeyExchange  
[ttls]     TLS_accept: SSLv3 read client key exchange A
[ttls] <<< TLS 1.0 ChangeCipherSpec [length 0001]  
[ttls] <<< TLS 1.0 Handshake [length 0010], Finished  
[ttls]     TLS_accept: SSLv3 read finished A
[ttls] >>> TLS 1.0 ChangeCipherSpec [length 0001]  
[ttls]     TLS_accept: SSLv3 write change cipher spec A
[ttls] >>> TLS 1.0 Handshake [length 0010], Finished  
[ttls]     TLS_accept: SSLv3 write finished A
[ttls]     TLS_accept: SSLv3 flush data
[ttls]     (other): SSL negotiation finished successfully
SSL Connection Established 
[ttls] eaptls_process returned 13 
++[eap] returns handled
Sending Access-Challenge of id 129 to 192.168.1.8 port 1645
	EAP-Message = 0x0106003d15800000003314030100010116030100282ff241f4503ca32dae130429d153ddf1fe80a7c7a39fe5c44150ea155c673a7a71fd09a9c3d9aecd
	Message-Authenticator = 0x00000000000000000000000000000000
	State = 0x11f1e0c914f7f53d9fb503cbe961a6a6
Finished request 14.
Going to the next request
Waking up in 4.6 seconds.
rad_recv: Access-Request packet from host 192.168.1.8 port 1645, id=130, length=201
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	User-Name = "wassim"
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
	State = 0x11f1e0c914f7f53d9fb503cbe961a6a6
	EAP-Message = 0x020600431500170301003897608bb651b1b252dc81ea0bdf3bb8e89500917999f419a7c03aac1dabb3a94b6d4008dc9f0fdb304bd36f7f79cbf659267a9d9b5288a1e4
	Message-Authenticator = 0xc2f48213dc59c560a1e64012ef16f00d
# Executing section authorize from file /etc/raddb/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 6 length 67
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/raddb/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/ttls
[eap] processing type ttls
[ttls] Authenticate
[ttls] processing EAP-TLS
[ttls] eaptls_verify returned 7 
[ttls] Done initial handshake
[ttls] eaptls_process returned 7 
[ttls] Session established.  Proceeding to decode tunneled attributes.
[ttls] Got tunneled request
	User-Name = "wassim"
	User-Password = "wassim"
	FreeRADIUS-Proxied-To = 127.0.0.1
[ttls] Sending tunneled request
	User-Name = "wassim"
	User-Password = "wassim"
	FreeRADIUS-Proxied-To = 127.0.0.1
	NAS-IP-Address = 192.168.1.8
	NAS-Port = 50023
	NAS-Port-Type = Ethernet
	Called-Station-Id = "00-15-F9-F8-4E-97"
	Calling-Station-Id = "00-1A-80-3F-F6-A1"
	Service-Type = Framed-User
	Framed-MTU = 1500
server inner-tunnel {
# Executing section authorize from file /etc/raddb/sites-enabled/inner-tunnel
+- entering group authorize {...}
++[chap] returns noop
++[mschap] returns noop
[suffix] No '@' in User-Name = "wassim", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
++[control] returns noop
[eap] No EAP-Message, not doing EAP
++[eap] returns noop
[files] users: Matched entry wassim at line 1
++[files] returns ok
[ldap] performing user authorization for wassim
[ldap] 	expand: %{Stripped-User-Name} -> 
[ldap] 	... expanding second conditional
[ldap] 	expand: %{User-Name} -> wassim
[ldap] 	expand: (uid=%{%{Stripped-User-Name}:-%{User-Name}}) -> (uid=wassim)
[ldap] 	expand: o=navbey.com, dc=navbey,dc=com -> o=navbey.com, dc=navbey,dc=com
  [ldap] ldap_get_conn: Checking Id: 0
  [ldap] ldap_get_conn: Got Id: 0
  [ldap] performing search in o=navbey.com, dc=navbey,dc=com, with filter (uid=wassim)
  [ldap] object not found
[ldap] search failed
  [ldap] ldap_release_conn: Release Id: 0
++[ldap] returns notfound
++[expiration] returns noop
++[logintime] returns noop
++[pap] returns updated
Found Auth-Type = PAP
# Executing group from file /etc/raddb/sites-enabled/inner-tunnel
+- entering group PAP {...}
[pap] login attempt with password "wassim"
[pap] Using clear text password "wassim"
[pap] User authenticated successfully
++[pap] returns ok
  WARNING: Empty post-auth section.  Using default return values.
# Executing section post-auth from file /etc/raddb/sites-enabled/inner-tunnel
} # server inner-tunnel
[ttls] Got tunneled reply code 2
	Tunnel-Medium-Type:1 = IEEE-802
	Tunnel-Type:1 = VLAN
	Tunnel-Private-Group-Id:1 = "100"
[ttls] Got tunneled Access-Accept
[eap] Freeing handler
++[eap] returns ok
# Executing section post-auth from file /etc/raddb/sites-enabled/default
+- entering group post-auth {...}
++[exec] returns noop
Sending Access-Accept of id 130 to 192.168.1.8 port 1645
	Tunnel-Medium-Type:1 = IEEE-802
	Tunnel-Type:1 = VLAN
	Tunnel-Private-Group-Id:1 = "100"
	MS-MPPE-Recv-Key = 0x483e4530dc779e0606078605d81146db8f3e24f896026c8b6785745b8765c8b6
	MS-MPPE-Send-Key = 0xd02414cb8e845d324e039e32acacfd91cff35fb428f8bc4a1af76c5bbacb69cf
	EAP-Message = 0x03060004
	Message-Authenticator = 0x00000000000000000000000000000000
	User-Name = "wassim"