Log of FreeRADIUS -X
Note: I tried different things here but I hope u can see the problem...

Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=231, length=262
        User-Name = "hausmeister"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02430060190017030100209a665b4a8764d353c69562eb7edb59b7d0a2723230256fee6cbcbee535c9fae017030100306b38cce4cff0c8f967cc84c2324f5e39303e9bec51026d0a47639f91df5c9d8a034b665f075d5af76dfb1cc33c7f392a
        State = 0x0f5577880b166e1916e506c906c4a85f
        Message-Authenticator = 0xc4591e579e2355ddf0b20dbfe3404c17
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "hausmeister", looking up realm NULL	
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 67 length 96
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] eaptls_verify returned 7
[peap] Done initial handshake
[peap] eaptls_process returned 7
[peap] EAPTLS_OK
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state WAITING FOR INNER IDENTITY
[peap] Identity - hausmeister
[peap] Got inner identity 'hausmeister'
[peap] Setting default EAP type for tunneled EAP session.
[peap] Got tunneled request
        EAP-Message = 0x0243001001686175736d656973746572
server  {
[peap] Setting User-Name to hausmeister
Sending tunneled request
        EAP-Message = 0x0243001001686175736d656973746572
        FreeRADIUS-Proxied-To = 127.0.0.1
        User-Name = "hausmeister"
server inner-tunnel {
# Executing section authorize from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authorize {...}
++[chap] returns noop
++[mschap] returns noop
[suffix] No '@' in User-Name = "hausmeister", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
++[control] returns noop
[eap] EAP packet type response id 67 length 16
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
++[pap] returns noop
WARNING: You set Proxy-To-Realm = LOCAL, but the realm does not exist!  Cancelling invalid proxy request.
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authenticate {...}
[eap] EAP Identity
[eap] processing type mschapv2
rlm_eap_mschapv2: Issuing Challenge
++[eap] returns handled
} # server inner-tunnel
[peap] Got tunneled reply code 11
        EAP-Message = 0x014400251a0144002010e97706b76512048df96d626e6edc500c686175736d656973746572
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x3b459b7d3b0181f6a0793e55cb6cf657
[peap] Got tunneled reply RADIUS code 11
        EAP-Message = 0x014400251a0144002010e97706b76512048df96d626e6edc500c686175736d656973746572
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x3b459b7d3b0181f6a0793e55cb6cf657
[peap] Got tunneled Access-Challenge
++[eap] returns handled
Sending Access-Challenge of id 231 to 192.168.2.135 port 32768
        EAP-Message = 0x0144004b1900170301004024fb98e1321a2dd6e2b2c384346674c184317bf895a65b60019b8f4aeb5f8096b7187349c6288ec89b420a423083069f33f7e2134286e3c993c3193436179cec
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x0f5577880a116e1916e506c906c4a85f
Finished request 13.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=232, length=310
        User-Name = "hausmeister"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02440090190017030100200c89f9d0fc24d6763aa95dbc31a8e5a6e3c2f45d54ba85f8febebdfcc08737dd17030100606115cf58b81da96fc04b409e8a45cd69f545d9fece14a89b423ba6915007946b6b9c48a09cdcafb61abb47c7cfbe7990ce873a5f003f1102fd971c8183f6cdad65659e5e47dce9cdc5fc6c548dde14c2226e6e0d0bcd00d3410d0f57d2952265
        State = 0x0f5577880a116e1916e506c906c4a85f
        Message-Authenticator = 0xfc92ec3967be4f9a8ca61bd908499b0f
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "hausmeister", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 68 length 144
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] eaptls_verify returned 7
[peap] Done initial handshake
[peap] eaptls_process returned 7
[peap] EAPTLS_OK
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state phase2
[peap] EAP type mschapv2
[peap] Got tunneled request
        EAP-Message = 0x024400461a02440041313582150b9fd390c4125511bd25c5ff2a0000000000000000368a4614a7753db7d1138525bfc0421be14c9375fa0d4cc900686175736d656973746572
server  {
[peap] Setting User-Name to hausmeister
Sending tunneled request
        EAP-Message = 0x024400461a02440041313582150b9fd390c4125511bd25c5ff2a0000000000000000368a4614a7753db7d1138525bfc0421be14c9375fa0d4cc900686175736d656973746572
        FreeRADIUS-Proxied-To = 127.0.0.1
        User-Name = "hausmeister"
        State = 0x3b459b7d3b0181f6a0793e55cb6cf657
server inner-tunnel {
# Executing section authorize from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authorize {...}
++[chap] returns noop
++[mschap] returns noop
[suffix] No '@' in User-Name = "hausmeister", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
++[control] returns noop
[eap] EAP packet type response id 68 length 70
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
++[pap] returns noop
WARNING: You set Proxy-To-Realm = LOCAL, but the realm does not exist!  Cancelling invalid proxy request.
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/mschapv2
[eap] processing type mschapv2
[mschapv2] # Executing group from file /etc/freeradius/sites-enabled/inner-tunnel
[mschapv2] +- entering group MS-CHAP {...}
[mschap] Creating challenge hash with username: hausmeister
[mschap] Told to do MS-CHAPv2 for hausmeister with NT-Password
[mschap]        expand: %{User-Name} -> hausmeister
[mschap]        expand: --username==%{%{User-Name}:-None}} -> --username==hausmeister}
Exec-Program output: Exec-Program: FAILED to execute /etc/freeradius/modules/ntlm_auth: Exec format error
Exec-Program-Wait: plaintext: Exec-Program: FAILED to execute /etc/freeradius/modules/ntlm_auth: Exec format error
Exec-Program: returned: 1
[mschap] External script failed.
[mschap] FAILED: MS-CHAP2-Response is incorrect
++[mschap] returns reject
[eap] Freeing handler
++[eap] returns reject
Failed to authenticate the user.
} # server inner-tunnel
[peap] Got tunneled reply code 3
        MS-CHAP-Error = "DE=691 R=1"
        EAP-Message = 0x04440004
        Message-Authenticator = 0x00000000000000000000000000000000
[peap] Got tunneled reply RADIUS code 3
        MS-CHAP-Error = "DE=691 R=1"
        EAP-Message = 0x04440004
        Message-Authenticator = 0x00000000000000000000000000000000
[peap] Tunneled authentication was rejected.
[peap] FAILURE
++[eap] returns handled
Sending Access-Challenge of id 232 to 192.168.2.135 port 32768
        EAP-Message = 0x0145002b190017030100200aea08094adbb43b6da707355b713535e3ac7e4402b398dd1c7ac9b1cee17843
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x0f55778809106e1916e506c906c4a85f
Finished request 14.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=233, length=246
        User-Name = "hausmeister"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02450050190017030100201654993f410953ea5e72bc3877bf247b1eb7ed34358b849bd0687248e947eb87170301002099e892137f466caa001f5d7c91f0313cf5a1248540e0e1c0e1d5ce59fae8da88
        State = 0x0f55778809106e1916e506c906c4a85f
        Message-Authenticator = 0x6c48466d9d95618004f406fb241fac08
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "hausmeister", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 69 length 80
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] eaptls_verify returned 7
[peap] Done initial handshake
[peap] eaptls_process returned 7
[peap] EAPTLS_OK
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state send tlv failure
[peap] Received EAP-TLV response.
[peap]  The users session was previously rejected: returning reject (again.)
[peap]  *** This means you need to read the PREVIOUS messages in the debug output
[peap]  *** to find out the reason why the user was rejected.
[peap]  *** Look for "reject" or "fail".  Those earlier messages will tell you.
[peap]  *** what went wrong, and how to fix the problem.
[eap] Handler failed in EAP/peap
[eap] Failed in EAP select
++[eap] returns invalid
Failed to authenticate the user.
Using Post-Auth-Type Reject
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group REJECT {...}
[attr_filter.access_reject]     expand: %{User-Name} -> hausmeister
attr_filter: Matched entry DEFAULT at line 11
++[attr_filter.access_reject] returns updated
Delaying reject of request 15 for 1 seconds
Going to the next request
Waking up in 0.9 seconds.
Sending delayed reject for request 15
Sending Access-Reject of id 233 to 192.168.2.135 port 32768
        EAP-Message = 0x04450004
        Message-Authenticator = 0x00000000000000000000000000000000
Waking up in 3.9 seconds.

#############################################

^Chaus-meister@KRATOS:/etc/freeradius/modules$ sudo freeradius -X
sudo: /var/lib/sudo/haus-meister durch nicht-Besitzer schreibbar (040777), sollte Modus 0700 haben
[sudo] password for haus-meister:
FreeRADIUS Version 2.1.12, for host x86_64-pc-linux-gnu, built on Feb 24 2014 at 14:57:57
Copyright (C) 1999-2009 The FreeRADIUS server project and contributors.
There is NO warranty; not even for MERCHANTABILITY or FITNESS FOR A
PARTICULAR PURPOSE.
You may redistribute copies of FreeRADIUS under the terms of the
GNU General Public License v2.
Starting - reading configuration files ...
including configuration file /etc/freeradius/radiusd.conf
including configuration file /etc/freeradius/proxy.conf
including configuration file /etc/freeradius/clients.conf
including files in directory /etc/freeradius/modules/
including configuration file /etc/freeradius/modules/pap
including configuration file /etc/freeradius/modules/sqlcounter_expire_on_login
including configuration file /etc/freeradius/modules/realm
including configuration file /etc/freeradius/modules/cui
including configuration file /etc/freeradius/modules/policy
including configuration file /etc/freeradius/modules/echo
including configuration file /etc/freeradius/modules/files
including configuration file /etc/freeradius/modules/acct_unique
including configuration file /etc/freeradius/modules/radutmp
including configuration file /etc/freeradius/modules/detail.log
including configuration file /etc/freeradius/modules/preprocess
including configuration file /etc/freeradius/modules/chap
including configuration file /etc/freeradius/modules/redis
including configuration file /etc/freeradius/modules/smsotp
including configuration file /etc/freeradius/modules/unix
including configuration file /etc/freeradius/modules/expiration
including configuration file /etc/freeradius/modules/linelog
including configuration file /etc/freeradius/modules/detail.example.com
including configuration file /etc/freeradius/modules/krb5
including configuration file /etc/freeradius/modules/attr_filter
including configuration file /etc/freeradius/modules/digest
including configuration file /etc/freeradius/modules/checkval
including configuration file /etc/freeradius/modules/replicate
including configuration file /etc/freeradius/modules/opendirectory
including configuration file /etc/freeradius/modules/smbpasswd
including configuration file /etc/freeradius/modules/inner-eap
including configuration file /etc/freeradius/modules/perl
including configuration file /etc/freeradius/modules/soh
including configuration file /etc/freeradius/modules/mac2vlan
including configuration file /etc/freeradius/modules/ippool
including configuration file /etc/freeradius/modules/expr
including configuration file /etc/freeradius/modules/etc_group
including configuration file /etc/freeradius/modules/ldap
including configuration file /etc/freeradius/modules/exec
including configuration file /etc/freeradius/modules/counter
including configuration file /etc/freeradius/modules/mschap
including configuration file /etc/freeradius/modules/detail
including configuration file /etc/freeradius/modules/passwd
including configuration file /etc/freeradius/modules/mac2ip
including configuration file /etc/freeradius/modules/rediswho
including configuration file /etc/freeradius/modules/logintime
including configuration file /etc/freeradius/modules/attr_rewrite
including configuration file /etc/freeradius/modules/otp
including configuration file /etc/freeradius/modules/ntlm_auth
including configuration file /etc/freeradius/modules/pam
including configuration file /etc/freeradius/modules/wimax
including configuration file /etc/freeradius/modules/sql_log
including configuration file /etc/freeradius/modules/always
including configuration file /etc/freeradius/modules/sradutmp
including configuration file /etc/freeradius/modules/dynamic_clients
including configuration file /etc/freeradius/eap.conf
including configuration file /etc/freeradius/policy.conf
including files in directory /etc/freeradius/sites-enabled/
including configuration file /etc/freeradius/sites-enabled/inner-tunnel
including configuration file /etc/freeradius/sites-enabled/default
main {
        user = "freerad"
        group = "freerad"
        allow_core_dumps = no
}
including dictionary file /etc/freeradius/dictionary
main {
        name = "freeradius"
        prefix = "/usr"
        localstatedir = "/var"
        sbindir = "/usr/sbin"
        logdir = "/var/log/freeradius"
        run_dir = "/var/run/freeradius"
        libdir = "/usr/lib/freeradius"
        radacctdir = "/var/log/freeradius/radacct"
        hostname_lookups = no
        max_request_time = 30
        cleanup_delay = 5
        max_requests = 1024
        pidfile = "/var/run/freeradius/freeradius.pid"
        checkrad = "/usr/sbin/checkrad"
        debug_level = 0
        proxy_requests = yes
 log {
        stripped_names = no
        auth = no
        auth_badpass = no
        auth_goodpass = no
 }
 security {
        max_attributes = 200
        reject_delay = 1
        status_server = yes
 }
}
radiusd: #### Loading Realms and Home Servers ####
 proxy server {
        retry_delay = 5
        retry_count = 3
        default_fallback = no
        dead_time = 120
        wake_all_if_all_dead = no
 }
 home_server localhost {
        ipaddr = 127.0.0.1
        port = 1812
        type = "auth"
        secret = "testing123"
        response_window = 20
        max_outstanding = 65536
        require_message_authenticator = yes
        zombie_period = 40
        status_check = "status-server"
        ping_interval = 30
        check_interval = 30
        num_answers_to_alive = 3
        num_pings_to_alive = 3
        revive_interval = 120
        status_check_timeout = 4
  coa {
        irt = 2
        mrt = 16
        mrc = 5
        mrd = 30
  }
 }
 home_server_pool my_auth_failover {
        type = fail-over
        home_server = localhost
 }
radiusd: #### Loading Clients ####
 client localhost {
        ipaddr = 127.0.0.1
        require_message_authenticator = no
        secret = "testing123"
        nastype = "other"
 }
 client 192.168.2.135 {
        require_message_authenticator = no
        secret = "testing123"
        shortname = "192.168.2.135"
 }
radiusd: #### Instantiating modules ####
 instantiate {
 Module: Linked to module rlm_exec
 Module: Instantiating module "exec" from file /etc/freeradius/modules/exec
  exec {
        wait = no
        input_pairs = "request"
        shell_escape = yes
  }
 Module: Linked to module rlm_expr
 Module: Instantiating module "expr" from file /etc/freeradius/modules/expr
 Module: Linked to module rlm_expiration
 Module: Instantiating module "expiration" from file /etc/freeradius/modules/expiration
  expiration {
        reply-message = "Password Has Expired  "
  }
 Module: Linked to module rlm_logintime
 Module: Instantiating module "logintime" from file /etc/freeradius/modules/logintime
  logintime {
        reply-message = "You are calling outside your allowed timespan  "
        minimum-timeout = 60
  }
 }
radiusd: #### Loading Virtual Servers ####
server { # from file /etc/freeradius/radiusd.conf
 modules {
  Module: Creating Auth-Type = digest
  Module: Creating Post-Auth-Type = REJECT
 Module: Checking authenticate {...} for more modules to load
 Module: Linked to module rlm_pap
 Module: Instantiating module "pap" from file /etc/freeradius/modules/pap
  pap {
        encryption_scheme = "auto"
        auto_header = no
  }
 Module: Linked to module rlm_chap
 Module: Instantiating module "chap" from file /etc/freeradius/modules/chap
 Module: Linked to module rlm_mschap
 Module: Instantiating module "mschap" from file /etc/freeradius/modules/mschap
  mschap {
        use_mppe = yes
        require_encryption = no
        require_strong = no
        with_ntdomain_hack = yes
        ntlm_auth = "/etc/freeradius/modules/ntlm_auth --request-nt-key --domain=OBLAN --username==%{%{User-Name}:-None}}"
        allow_retry = yes
  }
 Module: Linked to module rlm_digest
 Module: Instantiating module "digest" from file /etc/freeradius/modules/digest
 Module: Linked to module rlm_unix
 Module: Instantiating module "unix" from file /etc/freeradius/modules/unix
  unix {
        radwtmp = "/var/log/freeradius/radwtmp"
  }
 Module: Linked to module rlm_eap
 Module: Instantiating module "eap" from file /etc/freeradius/eap.conf
  eap {
        default_eap_type = "peap"
        timer_expire = 60
        ignore_unknown_eap_types = no
        cisco_accounting_username_bug = no
        max_sessions = 4096
  }
 Module: Linked to sub-module rlm_eap_md5
 Module: Instantiating eap-md5
 Module: Linked to sub-module rlm_eap_leap
 Module: Instantiating eap-leap
 Module: Linked to sub-module rlm_eap_gtc
 Module: Instantiating eap-gtc
   gtc {
        challenge = "Password: "
        auth_type = "PAP"
   }
 Module: Linked to sub-module rlm_eap_tls
 Module: Instantiating eap-tls
   tls {
        rsa_key_exchange = no
        dh_key_exchange = yes
        rsa_key_length = 512
        dh_key_length = 512
        verify_depth = 0
        CA_path = "/etc/freeradius/certs"
        pem_file_type = yes
        private_key_file = "/etc/freeradius/certs/server.key"
        certificate_file = "/etc/freeradius/certs/server.pem"
        CA_file = "/etc/freeradius/certs/ca.pem"
        private_key_password = "whatever"
        dh_file = "/etc/freeradius/certs/dh"
        random_file = "/dev/urandom"
        fragment_size = 1024
        include_length = yes
        check_crl = no
        cipher_list = "DEFAULT"
        make_cert_command = "/etc/freeradius/certs/bootstrap"
        ecdh_curve = "prime256v1"
    cache {
        enable = no
        lifetime = 24
        max_entries = 255
    }
    verify {
    }
    ocsp {
        enable = no
        override_cert_url = yes
        url = "http://127.0.0.1/ocsp/"
    }
   }
 Module: Linked to sub-module rlm_eap_ttls
 Module: Instantiating eap-ttls
   ttls {
        default_eap_type = "md5"
        copy_request_to_tunnel = no
        use_tunneled_reply = no
        virtual_server = "inner-tunnel"
        include_length = yes
   }
 Module: Linked to sub-module rlm_eap_peap
 Module: Instantiating eap-peap
   peap {
        default_eap_type = "mschapv2"
        copy_request_to_tunnel = no
        use_tunneled_reply = no
        proxy_tunneled_request_as_eap = yes
        virtual_server = "inner-tunnel"
        soh = no
   }
 Module: Linked to sub-module rlm_eap_mschapv2
 Module: Instantiating eap-mschapv2
   mschapv2 {
        with_ntdomain_hack = no
        send_error = no
   }
 Module: Checking authorize {...} for more modules to load
 Module: Linked to module rlm_preprocess
 Module: Instantiating module "preprocess" from file /etc/freeradius/modules/preprocess
  preprocess {
        huntgroups = "/etc/freeradius/huntgroups"
        hints = "/etc/freeradius/hints"
        with_ascend_hack = no
        ascend_channels_per_line = 23
        with_ntdomain_hack = no
        with_specialix_jetstream_hack = no
        with_cisco_vsa_hack = no
        with_alvarion_vsa_hack = no
  }
 Module: Linked to module rlm_realm
 Module: Instantiating module "suffix" from file /etc/freeradius/modules/realm
  realm suffix {
        format = "suffix"
        delimiter = "@"
        ignore_default = no
        ignore_null = no
  }
 Module: Linked to module rlm_files
 Module: Instantiating module "files" from file /etc/freeradius/modules/files
  files {
        usersfile = "/etc/freeradius/users"
        acctusersfile = "/etc/freeradius/acct_users"
        preproxy_usersfile = "/etc/freeradius/preproxy_users"
        compat = "no"
  }
 Module: Checking preacct {...} for more modules to load
 Module: Linked to module rlm_acct_unique
 Module: Instantiating module "acct_unique" from file /etc/freeradius/modules/acct_unique
  acct_unique {
        key = "User-Name, Acct-Session-Id, NAS-IP-Address, Client-IP-Address, NAS-Port"
  }
 Module: Checking accounting {...} for more modules to load
 Module: Linked to module rlm_detail
 Module: Instantiating module "detail" from file /etc/freeradius/modules/detail
  detail {
        detailfile = "/var/log/freeradius/radacct/%{%{Packet-Src-IP-Address}:-%{Packet-Src-IPv6-Address}}/detail-%Y%m%d"
        header = "%t"
        detailperm = 384
        dirperm = 493
        locking = no
        log_packet_header = no
  }
 Module: Linked to module rlm_radutmp
 Module: Instantiating module "radutmp" from file /etc/freeradius/modules/radutmp
  radutmp {
        filename = "/var/log/freeradius/radutmp"
        username = "%{User-Name}"
        case_sensitive = yes
        check_with_nas = yes
        perm = 384
        callerid = yes
  }
 Module: Linked to module rlm_attr_filter
 Module: Instantiating module "attr_filter.accounting_response" from file /etc/freeradius/modules/attr_filter
  attr_filter attr_filter.accounting_response {
        attrsfile = "/etc/freeradius/attrs.accounting_response"
        key = "%{User-Name}"
        relaxed = no
  }
 Module: Checking session {...} for more modules to load
 Module: Checking post-proxy {...} for more modules to load
 Module: Checking post-auth {...} for more modules to load
 Module: Instantiating module "attr_filter.access_reject" from file /etc/freeradius/modules/attr_filter
  attr_filter attr_filter.access_reject {
        attrsfile = "/etc/freeradius/attrs.access_reject"
        key = "%{User-Name}"
        relaxed = no
  }
 } # modules
} # server
server inner-tunnel { # from file /etc/freeradius/sites-enabled/inner-tunnel
 modules {
 Module: Checking authenticate {...} for more modules to load
 Module: Checking authorize {...} for more modules to load
 Module: Checking session {...} for more modules to load
 Module: Checking post-proxy {...} for more modules to load
 Module: Checking post-auth {...} for more modules to load
 } # modules
} # server
radiusd: #### Opening IP addresses and Ports ####
listen {
        type = "auth"
        ipaddr = *
        port = 0
}
listen {
        type = "acct"
        ipaddr = *
        port = 0
}
listen {
        type = "auth"
        ipaddr = 127.0.0.1
        port = 18120
}
 ... adding new socket proxy address * port 34959
Listening on authentication address * port 1812
Listening on accounting address * port 1813
Listening on authentication address 127.0.0.1 port 18120 as server inner-tunnel
Listening on proxy address * port 1814
Ready to process requests.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=234, length=176
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02a7001601686175736d656973746572404f424c414e
        Message-Authenticator = 0xd51f54ae5f9b17379fe3d511fec18d56
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 167 length 22
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
[pap] WARNING! No "known good" password found for the user.  Authentication may fail because of this.
++[pap] returns noop
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] EAP Identity
[eap] processing type tls
[tls] Initiate
[tls] Start returned 1
++[eap] returns handled
Sending Access-Challenge of id 234 to 192.168.2.135 port 32768
        EAP-Message = 0x01a800061920
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b8886260e60714841e768ed44c
Finished request 0.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=235, length=380
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02a800d01980000000c616030100c1010000bd030153e8e1ae795c570efdbf2887ee963a357797f8281ce7c8debcf217ebec133cf2000054c014c00ac022c02100390038c00fc0050035c012c008c01cc01b00160013c00dc003000ac013c009c01fc01e00330032c00ec004002fc011c007c00cc002000500040015001200090014001100080006000300ff01000040000b000403000102000a00340032000e000d0019000b000c00180009000a00160017000800060007001400150004000500120013000100020003000f00100011
        State = 0x88ca79b8886260e60714841e768ed44c
        Message-Authenticator = 0x43bbc89d240d99f020d12479bb8491b5
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 168 length 208
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
  TLS Length 198
[peap] Length Included
[peap] eaptls_verify returned 11
[peap]     (other): before/accept initialization
[peap]     TLS_accept: before/accept initialization
[peap] <<< TLS 1.0 Handshake [length 00c1], ClientHello
[peap]     TLS_accept: SSLv3 read client hello A
[peap] >>> TLS 1.0 Handshake [length 0039], ServerHello
[peap]     TLS_accept: SSLv3 write server hello A
[peap] >>> TLS 1.0 Handshake [length 02c0], Certificate
[peap]     TLS_accept: SSLv3 write certificate A
[peap] >>> TLS 1.0 Handshake [length 014b], ServerKeyExchange
[peap]     TLS_accept: SSLv3 write key exchange A
[peap] >>> TLS 1.0 Handshake [length 0004], ServerHelloDone
[peap]     TLS_accept: SSLv3 write server done A
[peap]     TLS_accept: SSLv3 flush data
[peap]     TLS_accept: Need to read more data: SSLv3 read client certificate A
In SSL Handshake Phase
In SSL Accept mode
[peap] eaptls_process returned 13
[peap] EAPTLS_HANDLED
++[eap] returns handled
Sending Access-Challenge of id 235 to 192.168.2.135 port 32768
        EAP-Message = 0x01a9040019c00000045c1603010039020000350301a02440262adabb19d9107106077625c7b61b329635cbdd4f41d5713c547c5c9700c01400000dff01000100000b00040300010216030102c00b0002bc0002b90002b6308202b23082019aa003020102020900f349c1d40d1d50ee300d06092a864886f70d01010b05003011310f300d060355040313064b5241544f53301e170d3134303830383135313933365a170d3234303830353135313933365a3011310f300d060355040313064b5241544f5330820122300d06092a864886f70d01010105000382010f003082010a0282010100d1b845087d1818ccf594d91354c4663ffd77f9594545494a
        EAP-Message = 0x6933a94d74204f387d09c538e6e60c89dc5c8c256b98ce525c7c347038f6e79c736123b95094166da4a72403511262399331362c9e71b9e93076be37c0309d861da4d8b68bd948886b70d079e322119a9fadd045347e1d0386ba46b3cd7e9520e9940f3ccdd802199e3f861259f33c8639cebef505dcc358a010500eee5ef0977b9ed0d88f2d34d0700609dd7d8512158daee745103f0efa9f0dd155bb4cf8377ce36d925ee67be0d94aba909b64f1d94166ce67c37b65d278c4f23013610c9f6c2bbf8db4a70a54d8f2e911028198ad48ee0ac6e6eb0bdbabc3218da98dfe041426194863057c7d0203010001a30d300b30090603551d130402300030
        EAP-Message = 0x0d06092a864886f70d01010b05000382010100af2e7a028d7cfb404264d1d5683102fc224d8a95a9a2a80240be4659011cbeb586de63d09f502569decb94c0a1f5971978603b623ac1c7f6e6b31cd4215881bae2dd8fa5839f45b982c9426c1dde971185eb1ae20253723bda27305a3b0a092dff0b9ffd8058b3eda1ae84f82992bdb92d5da75d1c2204cfd39fa990a20f2ae4072edc0cfbf0ff8a7bcd5221297611bcab8932757ff5fde368eabf75c85949b76850f5ab578a4423a78b5afe4e414f47fee7a1e18c074d87bd4072391e8f59fa976269a58fd6ed17d66fa25b6d5fb57bf75b9b73f2e59696a493fae910482922f4bac178cebe8c4be1fa
        EAP-Message = 0x69e8ce3b677364578ae436635b183425eaac1f02dc71160301014b0c00014703001741046d30070a80ae64ae49e5bc7f4dae826ba99838046b4baa0e336bf8a615470924206bd98ad2a2ed6f10882f9888b3a439a1331eb95612eb92ebdf022ff65ab7c80100c86c05b0bfe375c82c78dd996c54b2785e3836299e6c121523b5ff58cdd4870272744a631ff114abb6c56dd8d5686a087fa4c0939f79d65b2dc0d2287a5f93d94eb614afa2d817a4f896c6e7b5181a8d8a584d5e978fb94e3a40ed4b79172c97ff400182e82015f0c3b86930145bb409d0e31d384d8c87bdf7968bb48b62978c17fe0951ff10113af1b64f3bf1d9ffa38f5b54989af68b
        EAP-Message = 0x638596f6e478a286e00c9fbf
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b8896360e60714841e768ed44c
Finished request 1.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=236, length=178
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02a900061900
        State = 0x88ca79b8896360e60714841e768ed44c
        Message-Authenticator = 0x548b1aa7ac719189473f9f8c9e069f60
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 169 length 6
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] Received TLS ACK
[peap] ACK handshake fragment handler
[peap] eaptls_verify returned 1
[peap] eaptls_process returned 13
[peap] EAPTLS_HANDLED
++[eap] returns handled
Sending Access-Challenge of id 236 to 192.168.2.135 port 32768
        EAP-Message = 0x01aa006c1900eafb53fbd02ceeebb6e89b34321602dc7fa449628af9adea3bdcf9a6bcfe72e941ff7614511adaa10f8ba10531fd4de02d3274c9e242f2bda0a7466568d815c23857ba6ddca679ff87e35646a93fb5e9b03daeb28e1e73686708b37b3e16030100040e000000
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b88a6060e60714841e768ed44c
Finished request 2.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=237, length=316
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02aa009019800000008616030100461000004241045415ef5e9c4440b08e640593c7ba55d92bbbcc536e97f29db27d8387eae7d6cc8603099f8ec4766e87934dc4cb5d2f7f48fed2fab41ee980a1348742fa05f76f14030100010116030100306ae352ed5a69ad177fad937a106bedef39fff3d4fa1222a085c78c4e8532f5d695658b175f591b425c806d22ce08b46d
        State = 0x88ca79b88a6060e60714841e768ed44c
        Message-Authenticator = 0x75ce9b8e15b53b00ceeced4a22f9f659
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 170 length 144
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
  TLS Length 134
[peap] Length Included
[peap] eaptls_verify returned 11
[peap] <<< TLS 1.0 Handshake [length 0046], ClientKeyExchange
[peap]     TLS_accept: SSLv3 read client key exchange A
[peap] <<< TLS 1.0 ChangeCipherSpec [length 0001]
[peap] <<< TLS 1.0 Handshake [length 0010], Finished
[peap]     TLS_accept: SSLv3 read finished A
[peap] >>> TLS 1.0 ChangeCipherSpec [length 0001]
[peap]     TLS_accept: SSLv3 write change cipher spec A
[peap] >>> TLS 1.0 Handshake [length 0010], Finished
[peap]     TLS_accept: SSLv3 write finished A
[peap]     TLS_accept: SSLv3 flush data
[peap]     (other): SSL negotiation finished successfully
SSL Connection Established
[peap] eaptls_process returned 13
[peap] EAPTLS_HANDLED
++[eap] returns handled
Sending Access-Challenge of id 237 to 192.168.2.135 port 32768
        EAP-Message = 0x01ab00411900140301000101160301003097366ad90a60edfd983ce6b7bbca19853dc223d5485e3dd1f221d4cdd5b246bc8a7061b811c4596aafd27b6524e4e0e3
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b88b6160e60714841e768ed44c
Finished request 3.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=238, length=178
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02ab00061900
        State = 0x88ca79b88b6160e60714841e768ed44c
        Message-Authenticator = 0xb7f13b78b304e4b7966cfa22115df1fb
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 171 length 6
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] Received TLS ACK
[peap] ACK handshake is finished
[peap] eaptls_verify returned 3
[peap] eaptls_process returned 3
[peap] EAPTLS_SUCCESS
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state TUNNEL ESTABLISHED
++[eap] returns handled
Sending Access-Challenge of id 238 to 192.168.2.135 port 32768
        EAP-Message = 0x01ac002b1900170301002081d57c76a83ff27da706fedf2b710e49a623b42e9e22c47f0afa964182eead00
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b88c6660e60714841e768ed44c
Finished request 4.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=239, length=268
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02ac00601900170301002056dbe7183317514fda077476cadb313bbb6412d385f9d48ad0c5ffe80bf74e4917030100306f0f094ec69c62e45106d0e1c4bf6e66071de6dee8e07c28b46b8e41357a8f0616e07c21ed9d9a9004a26e3523e2079a
        State = 0x88ca79b88c6660e60714841e768ed44c
        Message-Authenticator = 0xf6e35547f122f4d1f0ea0b35da996fc9
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 172 length 96
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] eaptls_verify returned 7
[peap] Done initial handshake
[peap] eaptls_process returned 7
[peap] EAPTLS_OK
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state WAITING FOR INNER IDENTITY
[peap] Identity - hausmeister@OBLAN
[peap] Got inner identity 'hausmeister@OBLAN'
[peap] Setting default EAP type for tunneled EAP session.
[peap] Got tunneled request
        EAP-Message = 0x02ac001601686175736d656973746572404f424c414e
server  {
[peap] Setting User-Name to hausmeister@OBLAN
Sending tunneled request
        EAP-Message = 0x02ac001601686175736d656973746572404f424c414e
        FreeRADIUS-Proxied-To = 127.0.0.1
        User-Name = "hausmeister@OBLAN"
server inner-tunnel {
# Executing section authorize from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authorize {...}
++[chap] returns noop
++[mschap] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
++[control] returns noop
[eap] EAP packet type response id 172 length 22
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
++[pap] returns noop
WARNING: You set Proxy-To-Realm = LOCAL, but the realm does not exist!  Cancelling invalid proxy request.
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authenticate {...}
[eap] EAP Identity
[eap] processing type mschapv2
rlm_eap_mschapv2: Issuing Challenge
++[eap] returns handled
} # server inner-tunnel
[peap] Got tunneled reply code 11
        EAP-Message = 0x01ad002b1a01ad002610df95b54003dda3c224363ad05c6825f3686175736d656973746572404f424c414e
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0xe1eab64ee147ac5f275349b60dba1633
[peap] Got tunneled reply RADIUS code 11
        EAP-Message = 0x01ad002b1a01ad002610df95b54003dda3c224363ad05c6825f3686175736d656973746572404f424c414e
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0xe1eab64ee147ac5f275349b60dba1633
[peap] Got tunneled Access-Challenge
++[eap] returns handled
Sending Access-Challenge of id 239 to 192.168.2.135 port 32768
        EAP-Message = 0x01ad004b1900170301004064911e97ba196519cb1ff2c0f3b38ebf3b72f00166237a5c602d4a01d1e746bd0952cca525dd7f91646519ff82734b9593a7775e237a742eda78fe870e31132b
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b88d6760e60714841e768ed44c
Finished request 5.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=240, length=316
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02ad00901900170301002004fa09f0e1cfc2c609c101e3f93271ac01b87bbd04c7aaf4b749ec3660cd9df51703010060e556729273d866674b49a5d8fea84712645f0524e7820cf0d1e09d0064fc853cd7bf0c43d7f15b3dc75b516594162e8eb8b436c026923d72fce78e0d2ce263c71d42542e740cc589fdaa96996cc78cd01d72967b8cddc2000460ca40882e84f7
        State = 0x88ca79b88d6760e60714841e768ed44c
        Message-Authenticator = 0x045ba93626cfd0dfb19949c49cb563a8
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 173 length 144
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] eaptls_verify returned 7
[peap] Done initial handshake
[peap] eaptls_process returned 7
[peap] EAPTLS_OK
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state phase2
[peap] EAP type mschapv2
[peap] Got tunneled request
        EAP-Message = 0x02ad004c1a02ad004731a4528d68f36c5de70ff3905f73c6b15000000000000000006a5a977bbb28e2be9ad32289b3b0442f9043ff5d4465b69700686175736d656973746572404f424c414e
server  {
[peap] Setting User-Name to hausmeister@OBLAN
Sending tunneled request
        EAP-Message = 0x02ad004c1a02ad004731a4528d68f36c5de70ff3905f73c6b15000000000000000006a5a977bbb28e2be9ad32289b3b0442f9043ff5d4465b69700686175736d656973746572404f424c414e
        FreeRADIUS-Proxied-To = 127.0.0.1
        User-Name = "hausmeister@OBLAN"
        State = 0xe1eab64ee147ac5f275349b60dba1633
server inner-tunnel {
# Executing section authorize from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authorize {...}
++[chap] returns noop
++[mschap] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
++[control] returns noop
[eap] EAP packet type response id 173 length 76
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
++[pap] returns noop
WARNING: You set Proxy-To-Realm = LOCAL, but the realm does not exist!  Cancelling invalid proxy request.
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/inner-tunnel
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/mschapv2
[eap] processing type mschapv2
[mschapv2] # Executing group from file /etc/freeradius/sites-enabled/inner-tunnel
[mschapv2] +- entering group MS-CHAP {...}
[mschap] Creating challenge hash with username: hausmeister@OBLAN
[mschap] Told to do MS-CHAPv2 for hausmeister@OBLAN with NT-Password
[mschap]        expand: %{User-Name} -> hausmeister@OBLAN
[mschap]        expand: --username==%{%{User-Name}:-None}} -> --username==hausmeister@OBLAN}
Exec-Program output: Exec-Program: FAILED to execute /etc/freeradius/modules/ntlm_auth: Exec format error
Exec-Program-Wait: plaintext: Exec-Program: FAILED to execute /etc/freeradius/modules/ntlm_auth: Exec format error
Exec-Program: returned: 1
[mschap] External script failed.
[mschap] FAILED: MS-CHAP2-Response is incorrect
++[mschap] returns reject
[eap] Freeing handler
++[eap] returns reject
Failed to authenticate the user.
} # server inner-tunnel
[peap] Got tunneled reply code 3
        MS-CHAP-Error = "\255E=691 R=1"
        EAP-Message = 0x04ad0004
        Message-Authenticator = 0x00000000000000000000000000000000
[peap] Got tunneled reply RADIUS code 3
        MS-CHAP-Error = "\255E=691 R=1"
        EAP-Message = 0x04ad0004
        Message-Authenticator = 0x00000000000000000000000000000000
[peap] Tunneled authentication was rejected.
[peap] FAILURE
++[eap] returns handled
Sending Access-Challenge of id 240 to 192.168.2.135 port 32768
        EAP-Message = 0x01ae002b19001703010020d7308ed9a6c451aaaeaad80fb2530483903de5afdb20729fd9c5a6989748512b
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x88ca79b88e6460e60714841e768ed44c
Finished request 6.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=241, length=252
        User-Name = "hausmeister@OBLAN"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02ae0050190017030100206ef01542c9a142c8dc1371854db41feaa1716588c083b1c5baba75e2a1879fd51703010020d961f45859025d526fff9b0333d39cd0c09e06e648f7bd36eaa0a5fc533b26c3
        State = 0x88ca79b88e6460e60714841e768ed44c
        Message-Authenticator = 0x82a7bcbf6168ae5ceafb99994fafe07d
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "OBLAN" for User-Name = "hausmeister@OBLAN"
[suffix] No such realm "OBLAN"
++[suffix] returns noop
[eap] EAP packet type response id 174 length 80
[eap] Continuing tunnel setup.
++[eap] returns ok
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP/peap
[eap] processing type peap
[peap] processing EAP-TLS
[peap] eaptls_verify returned 7
[peap] Done initial handshake
[peap] eaptls_process returned 7
[peap] EAPTLS_OK
[peap] Session established.  Decoding tunneled attributes.
[peap] Peap state send tlv failure
[peap] Received EAP-TLV response.
[peap]  The users session was previously rejected: returning reject (again.)
[peap]  *** This means you need to read the PREVIOUS messages in the debug output
[peap]  *** to find out the reason why the user was rejected.
[peap]  *** Look for "reject" or "fail".  Those earlier messages will tell you.
[peap]  *** what went wrong, and how to fix the problem.
[eap] Handler failed in EAP/peap
[eap] Failed in EAP select
++[eap] returns invalid
Failed to authenticate the user.
Using Post-Auth-Type Reject
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group REJECT {...}
[attr_filter.access_reject]     expand: %{User-Name} -> hausmeister@OBLAN
attr_filter: Matched entry DEFAULT at line 11
++[attr_filter.access_reject] returns updated
Delaying reject of request 7 for 1 seconds
Going to the next request
Waking up in 0.9 seconds.
Sending delayed reject for request 7
Sending Access-Reject of id 241 to 192.168.2.135 port 32768
        EAP-Message = 0x04ae0004
        Message-Authenticator = 0x00000000000000000000000000000000
Waking up in 3.9 seconds.
Cleaning up request 0 ID 234 with timestamp +24
Cleaning up request 1 ID 235 with timestamp +24
Cleaning up request 2 ID 236 with timestamp +24
Cleaning up request 3 ID 237 with timestamp +24
Cleaning up request 4 ID 238 with timestamp +24
Cleaning up request 5 ID 239 with timestamp +24
Cleaning up request 6 ID 240 with timestamp +24
Waking up in 1.0 seconds.
Cleaning up request 7 ID 241 with timestamp +24
Ready to process requests.



####################################################
####################################################

Ready to process requests.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=243, length=164
        User-Name = "hausmeister"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02fe001001686175736d656973746572
        Message-Authenticator = 0xe530d9d420601a95ef9a91c9b1a4d4cc
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "hausmeister", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 254 length 16
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
[pap] WARNING! No "known good" password found for the user.  Authentication may fail because of this.
++[pap] returns noop
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] EAP Identity
[eap] processing type tls
[tls] Initiate
[tls] Start returned 1
++[eap] returns handled
Sending Access-Challenge of id 243 to 192.168.2.135 port 32768
        EAP-Message = 0x01ff00061920
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0xde5cee47dea3f7529bd8501b9c7793e7
Finished request 0.
Going to the next request
Waking up in 4.9 seconds.
rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=245, length=176
        User-Name = "OBLAN\\hausmeister"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02670016014f424c414e5c686175736d656973746572
        Message-Authenticator = 0xc1411999949e1fa1b51b997152ba0513
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] No '@' in User-Name = "OBLAN\hausmeister", looking up realm NULL
[suffix] No such realm "NULL"
++[suffix] returns noop
[eap] EAP packet type response id 103 length 22
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
[pap] WARNING! No "known good" password found for the user.  Authentication may fail because of this.
++[pap] returns noop
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] EAP Identity
[eap] processing type tls
[tls] Initiate
[tls] Start returned 1
++[eap] returns handled
Sending Access-Challenge of id 245 to 192.168.2.135 port 32768
        EAP-Message = 0x016800061920
        Message-Authenticator = 0x00000000000000000000000000000000
        State = 0x71b67e9b71de67f007aacdc8980a5626
Finished request 2.
Going to the next request
Waking up in 4.9 seconds.

rad_recv: Access-Request packet from host 192.168.2.135 port 32768, id=248, length=178
        User-Name = "hausmeister@oblan"
        NAS-IP-Address = 192.168.2.135
        NAS-Port = 0
        Called-Station-Id = "64-70-02-DF-6A-BA:OB-AIRLAN"
        Calling-Station-Id = "F0-27-65-89-E2-96"
        Framed-MTU = 1400
        NAS-Port-Type = Wireless-802.11
        Connect-Info = "CONNECT 0Mbps 802.11b"
        EAP-Message = 0x02ea00060334
        State = 0x187ea4021894bd238b684b194d94f231
        Message-Authenticator = 0xb8fffa84732d696d4a030c08672f915d
# Executing section authorize from file /etc/freeradius/sites-enabled/default
+- entering group authorize {...}
++[preprocess] returns ok
++[chap] returns noop
++[mschap] returns noop
++[digest] returns noop
[suffix] Looking up realm "oblan" for User-Name = "hausmeister@oblan"
[suffix] No such realm "oblan"
++[suffix] returns noop
[eap] EAP packet type response id 234 length 6
[eap] No EAP Start, assuming it's an on-going EAP conversation
++[eap] returns updated
++[files] returns noop
++[expiration] returns noop
++[logintime] returns noop
[pap] WARNING! No "known good" password found for the user.  Authentication may fail because of this.
++[pap] returns noop
Found Auth-Type = EAP
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group authenticate {...}
[eap] Request found, released from the list
[eap] EAP NAK
[eap] NAK asked for unsupported type 52
[eap] No common EAP types found.
[eap] Failed in EAP select
++[eap] returns invalid
Failed to authenticate the user.
Using Post-Auth-Type Reject
# Executing group from file /etc/freeradius/sites-enabled/default
+- entering group REJECT {...}
[attr_filter.access_reject]     expand: %{User-Name} -> hausmeister@oblan
attr_filter: Matched entry DEFAULT at line 11
++[attr_filter.access_reject] returns updated
Delaying reject of request 5 for 1 seconds
Going to the next request
Waking up in 0.9 seconds.

Sending delayed reject for request 5
Sending Access-Reject of id 248 to 192.168.2.135 port 32768
        EAP-Message = 0x04ea0004
        Message-Authenticator = 0x00000000000000000000000000000000
Waking up in 3.9 seconds.
Cleaning up request 4 ID 247 with timestamp +59
Waking up in 1.0 seconds.
Cleaning up request 5 ID 248 with timestamp +59
Ready to process requests.
